# B15F: Member List

B15F Member List

This is the complete list of members for B15F, including all inherited members.

abort(std::string msg) | B15F | static
abort(std::exception &ex) | B15F | static
activateSelfTestMode(void) | B15F |
analogRead(uint8_t channel) | B15F |
analogSequence(uint8_t channel_a, uint16_t *buffer_a, uint32_t offset_a, uint8_t channel_b, uint16_t *buffer_b, uint32_t offset_b, uint16_t start, int16_t delta, uint16_t count) | B15F |
analogWrite0(uint16_t port) | B15F |
analogWrite1(uint16_t port) | B15F |
BAUDRATE | B15F | static
delay_ms(uint16_t ms) | B15F |
delay_us(uint16_t us) | B15F |
digitalRead0(void) | B15F |
digitalRead1(void) | B15F |
digitalWrite0(uint8_t) | B15F |
digitalWrite1(uint8_t) | B15F |
discard(void) | B15F |
exec(std::string cmd) | B15F | static
getBoardInfo(void) | B15F |
getInstance(void) | B15F | static
getRegister(volatile uint8_t *adr) | B15F |
MSG_FAIL | B15F | static
MSG_OK | B15F | static
PRE | B15F |
pwmSetFrequency(uint32_t freq) | B15F |
pwmSetValue(uint8_t value) | B15F |
readDipSwitch(void) | B15F |
reconnect(void) | B15F |
RECONNECT_TIMEOUT | B15F | static
RECONNECT_TRIES | B15F | static
setAbortHandler(errorhandler_t func) | B15F | static
setRegister(volatile uint8_t *adr, uint8_t val) | B15F |
testConnection(void) | B15F |
testIntConv(void) | B15F |
WDT_TIMEOUT | B15F | static